For 1990-2009 cars

### Removal Procedure

1. Remove the rear door panel handle (3).

Release upwards with plastic wedge.

2. Remove the door handle panel cover (1).

Release with plastic wedge.

3. Loosen the rear door inner paneling.

Remove the 4 bolts.

4. Remove the rear door trim panel.

• | Release the 5 clips

• | Unhook the cable inside door handle (arrows).

• | Remove the door trim panel.

### Installation Procedure

1. Install the rear door trim panel.

• | Install the cable.

• | 5 clips

Caution: Refer to Fastener Caution in the Preface section.

2. Install the rear door trim panel. Install the 4 screws

Tighten
Tighten the 4 screws to 1.5 N·m (13 lb in).

3. Install the door pull handle cover.
4. Install the rear door panel handle.