For 1990-2009 cars

### Removal Procedure

1. Remove the trim from the front seat backrest.
2. Release the 2 covering caps (1).
3. Remove the 4 screws (arrows).
4. Remove the trim (2).

### Installation Procedure

1. Install the trim of the front seat backrest.

Caution: Refer to Fastener Caution in the Preface section.

2. Insert the trim.

Tighten
Tighten the 4 bolts to 3 N·m (26 lb in).

3. Install the 2 covering caps.