For 1990-2009 cars

## Sunshade Replacement Visor

### Removal Procedure

Remove the sunshade.

• | Remove the 2 bolts.

• | Disconnect the wiring harness plug.

• | Remove the sunshade from the support.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

Install the sunshade.

• | Connect the wiring harness plug.

• | Install the sunshade into the main bracket.

• | Tighten the 2 bolts.

Tighten
Tighten the 2 bolts to 2.2 N·m (19 lb in).

## Sunshade Replacement Visor Cover

### Removal Procedure

1. Remove the sunshade cover (1).
2. Remove the 2 clips.

### Installation Procedure

1. Install the sunshade cover.
2. Install the 2 clips.