For 1990-2009 cars

### Removal Procedure

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement .
2. Remove the front fascia outer supports.

Drill out the 3 blind rivets (1).

3. Take off the front fascia outer supports.

### Installation Procedure

1. Prepare the front fascia outer supports.
2. Install the front fascia outer supports.

Rivet on the 4 blind rivets.

3. Attach the front bumper fascia. Refer to Front Bumper Fascia Replacement .