For 1990-2009 cars

### Removal Procedure

1. Remove the hood closure stud.

Remove the stud assembly.

2. Disassemble the hood closure stud (4).

• | Remove the disc nut (1).

• | Remove the coil spring (2) and washer (3) off of the stud.

### Installation Procedure

1. Install the hood closure stud (4).

• | Install the washer (3) and coil spring (2).

• | Install the disc nut (1).

• | Note the basic setting.

Specification
X = 43 /-3 mm (1.69/-0.11 in)

Notice: Refer to Fastener Notice in the Preface section.

2. Install the hood closure stud.

| Important: Remember to grease stud.

• | Install the stud assembly.

• | Lock the disc nut with the stud.

Tighten
Tighten the disc nut to 22 N·m (16 lb ft).