For 1990-2009 cars

### Removal Procedure

1. Remove the front floor console. Refer to Front Floor Console Replacement .
2. Remove the instrument panel (I/P) bracket - right side.

2.1. | Remove the 2 bolts (arrows).

2.2. | Remove the I/P retainer (1).

### Installation Procedure

1. Install the I/P retainer, right side.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the I/P retainer.

Tighten
Tighten the 2 bolts to 13 N·m (113 lb in).

3. Install the front floor console. Refer to Front Floor Console Replacement .