For 1990-2009 cars

#### Special Tools

KM-6625 Flywheel Locking

For equivalent regional tools, refer to Special Tools.

1. Using the KM-6625 locking , block the crankshaft from rotating.

1.1. | Detach the screwed connection (1).

1.2. | Insert the KM-6625 locking (2).

1.3. | Tighten the screwed connection (3).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the crankshaft balancer (1) and bolt (2).

2.1. | Tighten the bolt to 95 N·m (70 lb ft) - first pass.

2.2. | Tighten the bolt 45 degrees + 15 degrees - second pass