For 1990-2009 cars

### Removal Procedure

1. Remove the compressor. Refer to Air Conditioning Compressor Replacement.
2. Remove the compressor pulley. Refer to Air Conditioning Compressor Pulley Replacement.
3. Remove the clutch coil.

• | Release the wiring harness for clutch coil of compressor (2).

• | Remove the bolt.

• | Remove the retaining ring (1).

• | Remove the clutch coil off compressor.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

Note: When installing the compressor clutch coil, ensure correct seating of detent.

1. Install the clutch coil.

1.1. | Position the clutch coil.

1.2. | Insert the retaining ring.

1.3. | Connect the wiring harness.

Tighten
Tighten the bolt to 4 N·m (35 lb in).

2. Install the compressor pulley. Refer to Air Conditioning Compressor Pulley Replacement.
3. Install the compressor. Refer to Air Conditioning Compressor Replacement.