For 1990-2009 cars

## Tail Lamp Wiring Harness Replacement Coupe

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

Important: Replace or repair the wiring harnesses observing the safety regulations of electrics/electronics.

1. Disconnect the battery.
2. Remove the rear compartment, side trim panel, both sides. Refer to Rear Compartment Side Trim Panel Replacement .
3. Remove the wiring harness, rear end panel.

• | Disconnect the 7 wiring harness plugs.

• | Disconnect the ground connection.

• | Remove the nut.

• | Release the 16 clips.

• | Remove the wiring harness.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the wiring harness, rear end panel.

• | Position the wiring harness.

• | Install the 16 clips.

• | Connect the ground connection.

Tighten
Tighten the nut to 5 N·m (44 lb in).

• | Connect the 7 wiring harness plugs.

2. Install the rear compartment, side trim panel, both sides. Refer to Rear Compartment Side Trim Panel Replacement .
3. Connect the battery.
4. For reprogramming procedures, refer to Control Module References .

## Tail Lamp Wiring Harness Replacement Sedan

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

Important: Replace or repair wiring harnesses observing the safety regulations of electric/electronics.

1. Disconnect the battery.
2. Remove the rear compartment side panel. Refer to Rear Compartment Side Trim Panel Replacement .
3. Remove the wiring harness, rear end panel.

• | Disconnect the 7 wiring harness plugs.

• | Disconnect the ground connection.

• | Remove the nut.

• | Release the 16 clips.

• | Remove the wiring harness.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the wiring harness, rear end panel.

• | Position the wiring harness.

• | Install the 16 clips.

• | Connect the ground connection.

Tighten
Tighten the nut to 5 N·m (44 lb in).

• | Connect the 7 wiring harness plugs.

2. Install the rear compartment side panel. Refer to Rear Compartment Side Trim Panel Replacement .
3. Connect the battery.
4. For reprogramming procedures, refer to Control Module References .