For 1990-2009 cars

### Removal Procedure

1. Remove the front floor console. Refer to Front Floor Console Replacement.
2. Remove the instrument panel (I/P) retainer - left side.

• | Remove the 2 bolts (arrows).

• | Remove the I/P retainer (1).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the I/P retainer, left side.

Tighten
Tighten the 4 bolts to 13 N·m (113 lb in).

2. Install the front floor console. Refer to Front Floor Console Replacement.