For 1990-2009 cars

### Removal Procedure

1. Position the front seat to the rearmost position.
2. Remove the clutch pedal cruise control switch.

2.1. | Disconnect the wiring harness plug (1).

2.2. | Release the switch (2).

2.3. | Remove the switch fuse (3) in the direction of the arrow.

### Installation Procedure

1. Install the clutch pedal cruise control switch.

1.1. | Connect the wiring harness plug.

1.2. | Install the switch.

1.3. | Install the fuse.

2. Reposition the front seat to the original position.