For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Open the hood.
2. Disconnect the battery.

• | Remove the ground connection from the ground terminal.

• | Loosen the nut.

3. Raise the vehicle by its full height.
4. Remove the ground cable (1) from starter.

Remove the nut.

5. Remove the 2 positive cable (2) starter.

Remove the 2 nuts.

6. Remove the intake manifold bracket (2).

• | Disconnect the wiring harness plug of the catalytic converter control oxygen sensor.

• | Disconnect the wiring harness plug (1) from the bracket.

• | Remove the 2 bolts (3).

7. Remove the starter.

Remove the 2 bolts (1, 2).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the starter.

Tighten
Tighten the 2 bolts to 25 N·m (18 lb ft).

2. Install the intake manifold bracket.

Tighten
Tighten the 2 bolts to 8 N·m (70 lb in).

• | Install the wiring harness plug into the bracket.

• | Connect the wiring harness plug for the catalytic converter control oxygen sensor.

3. Install the wiring harness to the starter.

Tighten
Tighten the 2 nuts to 12.5 N·m (110 lb in).

4. Install the ground cable to the starter.

Tighten
Tighten the nut to 12.5 N·m (110 lb in).

5. Lower the vehicle by its full height.
6. Connect the battery.

Install the ground connection to the ground terminal.

Tighten
Tighten the nut to 12.5 N·m (110 lb in).

7. For programming procedures, refer to Control Module References .
8. Close the hood.