For 1990-2009 cars

### Removal Procedure

Remove the instrument panel (I/P) insulator panel.

• | Remove the 2 retainers (1) on the driver side and remove the I/P insulator from the bracket.

• | Remove the 2 retainers (2) on the passenger side and remove the I/P insulator from the bracket.

### Installation Procedure

Install the I/P insulator panel.

• | Insert the I/P insulator in the bracket and install the 2 retainers.

• | Insert the I/P insulator in the bracket and install the 2 retainers.