For 1990-2009 cars

1. Remove the sleeve/bore plug retainer (382) and the primary regulator valve sleeve (376).
2. Remove the primary regulator valve plunger (377), valve spring (378) and the primary regulator valve (379).
3. Remove the sleeve/bore plug retainer (382) and the accumulator regulator valve sleeve (396).
4. Remove the accumulator regulator valve plunger (397), valve spring (398) and the accumulator regulator valve (399).
5. Remove the sleeve/bore plug retainer (382) and the solenoid B-1 modulator valve no. 1 sleeve (395).
6. Remove the solenoid B-1 modulator valve no. 1 (394).
7. Remove the solenoid B-1 modulator valve no. 1 spring (393) and the solenoid B-1 modulator valve no. 1 plunger (392).
8. Remove the sleeve/bore plug retainer (382) and valve bore plug (383)
9. Remove the lock up control solenoid spring (381).
10. Remove the lock up control solenoid valve (380).
11. Remove the sleeve/bore plug retainer (382) and the valve bore plug (384).
12. Remove the 3-4 shift valve sleeve (385) and the 3-4 shift valve spring (386).
13. Remove the 3-4 shift valve spring (386) and the 3-4 shift valve (387).
14. Remove the sleeve/bore plug retainer (382) and the valve bore plug (383).
15. Remove the 2-3 shift valve spring (388) and the 2-3 shift valve (389).
16. Remove the sleeve/bore plug retainer (382) and the valve bore plug (383).
17. Remove the 1-2 shift valve (390) and the 1-2 shift valve spring (391).