For 1990-2009 cars

### Removal Procedure

1. Remove the radiator grille.

1.1. | Remove the 4 bolts (1).

1.2. | Release the 6 brackets (2).

2. Remove the radiator grille panel.

Remove the 16 clips.

### Installation Procedure

1. Install the radiator grille panel.

Install the 16 clips.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the radiator grille.

Install the 6 retainers.

Tighten
Tighten the 4 bolts to 2.5 N·m (22 lb in).