For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Remove the mass airflow sensor.
3. Disconnect the wiring harness plug (2).
4. Remove the 2 clamps (1).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the mass airflow sensor.

Tighten
Tighten the 2 clamps to 3.5 N·m (31 lb in).

2. Install the wiring harness plug.
3. Close the hood.