For 1990-2009 cars

### Removal Procedure

1. Remove the windshield air inlet screen (1).
2. Remove the wiper arms (2).

• | Remove the 2 covers.

• | Remove the 2 nuts.

• | Remove the 2 washers.

• | Remove the 2 windshield wiper arms from the shaft.

3. Remove the horn.

• | Remove the nut (1).

• | Disconnect the wiring harness plug (2).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the horn.

Connect the wiring harness plug.

Tighten
Tighten the nut to 5 N·m (44 lb in).

2. Install the windshield air inlet screen.

• | Install the hose for the windshield wash system.

• | Install the 5 clips.

3. Install the windshield wiper arms.

| Note: Ensure correct installation position of the windshield wiper arms.

• | Position the 2 windshield wiper arms on the shaft.

• | Install the 2 washers.

Tighten
Tighten the 2 nuts to 17 N·m (13 lb ft).

• | Install the 2 covers.

4. Install the windshield air inlet screen.