For 1990-2009 cars

### Removal Procedure

Important: The panel cannot be removed without damage and must be replaced.

1. Remove the door sill nameplate (1).
2. Remove the sill nameplate with a plastic wedge.

### Installation Procedure

Important: The adhesive surface must be free of dirt and grease.

1. Clean the surface to be bonded.
2. Pull off the protective film.
3. Install the door sill nameplate.