For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle.
2. Remove the wiring harness of the barometric pressure sensor (1).

• | Remove the wiring harness plug (2).

• | Remove the 1 or 2 cable ties (3).

3. Remove the barometric pressure sensor (1).

Remove the bolt (2).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the barometric pressure sensor.

Tighten
Tighten the bolt to 5 N·m (44 lb in).

2. Install the wiring harness of the barometric pressure sensor.

• | Install the wiring harness plug.

• | Install the cable ties.

3. Lower the vehicle.