For 1990-2009 cars

### Removal Procedure

1. Remove the combined tail lamp.

• | Open the access panel.

• | Remove the 2 bolts (2).

• | Remove the tail lamp circuit board.

• | Disconnect the wiring harness plug (1).

2. Remove the tail lamp holder.

Release the 4 clips (1).

3. Transfer the necessary tail lamp components.

### Installation Procedure

Important: Retaining clips must engage audibly.

1. Install the bulb holder.

Install the 4 clips.

Important:

• | Before installing the tail lamp, ensure that the tail lamp gasket is seated correctly.

• | The gasket (1) with the flat side must not be confused with the gasket (3).

2. Install the gasket (2).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the tail lamp circuit board.

• | Connect wiring harness plug.

• | Insert tail lamp circuit board.

• | Close the access panel.

Tighten
Tighten the 2 screws to 5 N·m (44 lb in).