For 1990-2009 cars

### Removal Procedure

1. Remove the rear side door regulator. Refer to Rear Side Door Window Regulator Replacement.
2. Remove the motor from the window regulator.

Remove the 3 bolts (1).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the motor to the window regulator.

Tighten
Tighten the 3 bolts to 3.5 N·m (32 lb in).

2. Install the rear side door regulator. Refer to Rear Side Door Window Regulator Replacement.