For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle by its full height.
2. Remove the engine rear mount.

• | Remove the 3 screwed connections (1, 2).

• | Remove the engine rear mount (3).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

Important: Ensure that the groove (3) engages in the recess (2).

1. Install the engine rear mount to the bracket with a new nut.

Tighten
Tighten the screwed joint to 55 N·m (40 lb ft).

2. Install the engine rear mount to the front frame with new nuts.

Tighten
Tighten the 2 screwed joints to 55 N·m (40 lb ft).

3. Lower the vehicle by its full height.