For 1990-2009 cars

### Removal Procedure

1. Remove the door sill plate.

• | Loosen the 5 clips.

• | Remove the sill plate upwards.

2. Remove the lower center pillar trim.

• | Loosen the upper center pillar trim in lower area and remove the lower center pillar.

• | Remove the center pillar trim.

• | Release the 4 clips.

### Installation Procedure

1. Install the lower center pillar trim.

• | Place the center pillar trim, install the upper center pillar trim in the lower center pillar.

• | Install the 4 clips.

2. Install the door sill plate.

Install the 5 clips.