For 1990-2009 cars

### Removal Procedure

1. Remove the transmission shifter opening trim. Refer to Front Floor Console Transmission Shift Opening Trim Plate Replacement.
2. Remove the front ashtray. Refer to Front Floor Console Front Ashtray Replacement.
3. Remove the range selector cable (2) from the range selector lever.

• | Remove the retaining clamp (1).

• | Disconnect the selector lever cable from the bracket.

Warning: Refer to Battery Disconnect Warning in the Preface section.

4. Remove the battery.

• | Disconnect the negative cable (2) from the battery.

| Remove the nut.

• | Disconnect the positive cable (3) from the battery.

| Remove the nut.

• | Remove the bracket (1).

| Remove the bolt (4).

5. Remove the battery tray.

• | Release the cable tie.

• | Remove the 3 bolts (1).

6. Remove the range selector cable from the transmission.

• | Remove from the selector lever position switch.

• | Remove from the bracket on the transmission.

• | Remove the retaining clamp (1).

7. Remove the range selector cable from the wiring harness.

Release the 2 brackets (2).

Note: Do not remove rubber seal from the dash.

8. Remove the range selector cable from the rubber seal (3).

### Installation Procedure

Note: Do not push rubber seal (3) into the dash.

1. Insert the range selector cable into the dash.

Coat the selector cable with soap solution.

2. Install the range selector cable to the transmission.

• | Install the range selector lever position switch.

• | Install range selector lever position switch to the bracket on the transmission.

• | Attach the retaining clamp (1).

3. Install the selector cable to the wiring harness.

Insert into the 2 brackets (2).

4. Install the selector cable (2) to the selector lever.

• | Install the selector lever cable to the bracket.

• | Install the retaining clamp (1).

5. Adjust the range selector cable. Refer to Range Selector Lever Cable Adjustment.
6. Install the front ashtray. Refer to Front Floor Console Front Ashtray Replacement.
7. Install the transmission shifter opening trim. Refer to Front Floor Console Transmission Shift Opening Trim Plate Replacement.

Caution: Refer to Fastener Caution in the Preface section.

8. Install the battery tray support.

Fasten the cable tie.

Tighten
Tighten the 3 bolts (1) to 10 N·m (89 lb in).

9. Install the battery.

• | Install the bracket (1).

Tighten
Tighten the bolt (4) to 15 N·m (11 lb ft).

• | Connect the positive cable (3) to the battery.

• | Connect the negative cable (2) to the battery.

10. For programming procedures, refer to Control Module References.
11. Inspect the selector lever for proper functions.