For 1990-2009 cars

#### Special Tools

J 39637 KM-6626 Wiper Arm Puller

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the battery.
2. Remove the windshield air inlet screen (1).
3. Remove the wiper arms (2).

• | Remove the 2 covers.

• | Remove the 2 nuts.

• | Remove the 2 washers.

• | Remove the wiper arm using J 39637 / KM-6626.

• | Disconnect the hose for the washer/wiper system.

4. Remove the windshield air inlet screen (1).

• | Lift the windshield air inlet screen in the vicinity of the dash.

| Note: Carefully release the clips from the inside from the upper dash.

• | Release the 5 clips (3).

• | Remove the hose for the air inlet screen (2).

5. Remove the power horn.

• | Disconnect the wiring harness plug (1).

• | Remove the 2 nuts (2).

• | Remove the power horn.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the power horn.

• | Position the power horn.

Tighten
Tighten the 2 nuts to 5 N·m (44 lb in).

• | Connect the wiring harness plug.

2. Install the windshield air inlet screen.

• | Install the hose to the air inlet screen.

• | Install the 5 clips.

3. Install the windshield wiper arms.

| Note: Ensure correct installation position of the windshield wiper arms.

• | Position the 2 windshield wiper arms on the shaft.

• | Install the 2 washers.

Tighten
Tighten the 2 nuts to 17 N·m (13 lb ft).

• | Install the 2 covers.

4. Install the windshield air inlet screen.
5. Connect the battery.
6. For reprogramming procedures, refer to Control Module References.