For 1990-2009 cars

### Removal Procedure

1. Remove the armrest.

Release from the guide.

2. Loosen the pad (1) under the central armrest.

Remove from the guide.

3. Remove the rear seat backrest flap (4).

• | Drive out 2 bush (3).

• | Remove 2 body-bound rivets (2).

### Installation Procedure

1. Install the rear seat backrest flap.

• | Insert 2 body-bound rivets.

• | Drive in 2 bush.

2. Fasten the pad under the central armrest.

Insert into the guide.

3. Install the armrest.

Clip in the guide.