For 1990-2009 cars

### Removal Procedure

Important: If the selector lever is not in the P position when the vehicle is left standing for a long period the battery can run flat. To prevent the battery from discharging, always remove the ignition key from the ignition lock when leaving for a period, including overnight.

1. Carefully remove the selector lever boot (1) from the selector lever cover.

Slide the boot upwards.

2. Release the selector lever.

• | Use a suitable tool to push the release lever (2) on the selector lever lock solenoid switch forwards (arrow) and hold in this position.

• | Press the lock control on the selector lever and disengage the selector lever from the P position.

### Installation Procedure

Clip the selector lever boot into the selector lever cover.