For 1990-2009 cars

### Removal Procedure

Important: Pull down (arrow) on the right-hand side of the interior dome lamp (1).

1. Remove the rear interior dome lamp.

Release the rear interior dome lamp.

2. Disconnect the wiring harness plug.
3. Remove the bulbs.

• | Release the locking plate (1).

• | Remove the 2 bulbs (2).

### Installation Procedure

1. Install the bulbs.

• | Install the 2 bulbs.

• | Close the locking plate.

2. Connect the wiring harness plug.
3. Install the rear interior dome lamp.