For 1990-2009 cars

### Removal Procedure

Remove the roof rail stowage compartment headlining.

1. Open the access panel (arrow).
2. Remove the 2 bolts.

### Installation Procedure

Install the roof rail stowage compartment headlining.

Caution: Refer to Fastener Caution in the Preface section.

1. Tighten the 2 bolts

Tighten
Tighten the 2 bolts to 2.8 N·m (25 lb in).

2. Close the access panel.