For 1990-2009 cars

#### Special Tools

KM-569-A Plug Remover

### Removal Procedure

1. Position the transmission control lever into 4th gear.
2. Remove the battery tray. Refer to Battery Tray Replacement .
3. Release the selector lever.

Important: Do not remove the bolt.

4. Loosen the bolt (1) for the relay point clamp.
5. Disconnect the transmission rocker arm from the relay point bracket.
6. Disconnect the 2 retaining clamps (1, 2) from the transmission rocker arm.
7. Disconnect the selector lever from the universal joint.

• | Press in retaining spring (arrow) of the hollow pin (3).

• | Detach the hollow pin with KM-569-A .

### Installation Procedure

Important: Use new retaining clamps.

1. Connect the transmission rocker arm to the relay point bracket.

Connect the 2 retaining clamps (1, 2) to the transmission rocker arm.

Important: Use a new hollow pin. Retaining spring (arrow) of hollow pin (3) must engage.

2. Connect the selector lever to the universal joint.

Connect a hollow pin.

3. Connect the selector lever to relay point.

Important: Do not tighten bolt (1) yet.

4. Install battery tray. Refer to Battery Tray Replacement .
5. Adjust the transmission shift linkage. Refer to Selector Lever Link Adjustment .
6. For programming procedures, refer to Control Module References .