For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Distributor Housing to Dash Bolt | 6 N·m | 53 lb in
Air Duct Brace Bolt - Left | 13 N·m | 113 lb in
Air Duct Brace Bolt - Right | 13 N·m | 113 lb in
Air Filter Bolt | 5 N·m | 44 lb in
Air Filter Cover Bolt | 2.5 N·m | 22 lb in
Block Connector Bolt | 7 N·m | 62 lb in
Blower Motor Bolt | 6 N·m | 63 lb in
Center Console Bracket Bolt - right | 13 N·m | 113 lb in
Center Instrument Panel (I/P) Bracket Bolt | 13 N·m | 113 lb in
Clutch Coil Bolt | 4 N·m | 35 lb in
Compressor Clutch Bolt | 12 N·m | 106 lb in
Compressor Hose Bolt | 20 N·m | 15 lb ft
Compressor to Main Bracket Bolt | 22 N·m | 16 lb ft
Condensation Drain Bolt | 5 N·m | 44 lb in
Condenser Bolt | 8 N·m | 71 lb in
Drain Hose Nut | 5 N·m | 44 lb in
Drain Hose to Dash Bolt | 5 N·m | 44 lb in
Engine Splash Shield Bolt | 8 N·m | 71 lb in
Evaporator Cover Bolt | 2.5 N·m | 22 lb in
Evaporator Hose Bolt | 20 N·m | 15 lb ft
Expansion Valve Bolt | 6 N·m | 53 lb in
Heater Core Cover Bolt | 6 N·m | 53 lb in
Heater Fan Motor Bolt | 8 N·m | 71 lb in
High Pressure Relief Valve | 10 N·m | 89 lb in
I/P Compartment Bolt | 4 N·m | 35 lb in
I/P Padding Bolt | 3 N·m | 26 lb in
I/P Tie Bar Bolt | 13 N·m | 113 lb in
Pressure Sensor | 10 N·m | 89 lb in
Pressure Sensor to Condenser | 10 N·m | 89 lb in
Recirculating Air Valve Housing Bolt | 5 N·m | 44 lb in
Recirculating Air Valve Housing Grille Bolt | 5 N·m | 44 lb in
Refrigerant Lines to Condenser Bolt | 20 N·m | 15 lb ft
Sealing Ring Bolt | 20 N·m | 15 lb ft
Service Port Valve Core | 2.5 N·m | 22 lb in
Windshield Wiper Arm Nut | 17 N·m | 13 lb ft
Wiper Arm Nut | 17 N·m | 13 lb ft
Wiper Arm to Shaft Nut | 17 N·m | 13 lb ft
Wiring Harness Plug Bolt | 5 N·m | 44 lb in