For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (I/P) compartment.

1.1. | Open the I/P compartment cover.

1.2. | Remove the 4 bolts (1).

1.3. | Disconnect the wiring harness plug.

1.4. | Remove the I/P compartment.

2. Support the I/P compartment door damper.

2.1. | Release the fastening clip (1).

2.2. | Remove the damper.

3. Release and remove the I/P compartment door.

3.1. | Remove the 2 bolts (2).

3.2. | Remove the I/P compartment door.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the I/P compartment door.

Tighten
Tighten the 2 bolts to 2.5 N·m (22 lb in).

2. Install the I/P compartment door damper.

Install the fastening clamp.

3. Install the I/P compartment.

3.1. | Connect the wiring harness plug.

3.2. | Insert the I/P compartment.

Tighten
Tighten the 4 bolts to 4 N·m (35 lb in).

3.3. | Close the I/P compartment door.