For 1990-2009 cars

## Door Bottom Auxiliary Sealing Strip Replacement Sedan

### Removal Procedure

1. Open the front and rear doors.

Important: Release with an appropriate tool (1).

2. Release the door button sealing strip.

Release the 10 rivets (arrows).

### Installation Procedure

1. Install the door button sealing strip.

Install the 10 clips.

2. Close the front and rear doors.

## Door Bottom Auxiliary Sealing Strip Replacement Coupe

### Removal Procedure

1. Remove the door button sealing strip.
2. Remove the 7 rivet heads from the outer the sill paneling.

### Installation Procedure

1. Install the door button sealing strip.
2. Install the 7 rivet heads to the outer sill paneling.