For 1990-2009 cars

#### Special Tools

• | J 26941 Bushing and Bearing Remover - 3-4 in

• | SA9133T Axle Seal Puller

• | SA9133T-1 Axle Seal Puller Adapter

1. Remove the 1 lube fluid pipe retainer bolt (804) and the lube fluid pipe retainer (803) from the torque converter housing (10).

Important: Be careful not to damage the lube fluid pipe.

2. Remove the lube fluid pipe (805).
3. Remove the 3 fluid baffle bolts (810) and the transmission fluid baffle (811).
4. Remove the 3 chip collector magnets (812) from the fluid baffle (811).
5. Using a hammer and screwdriver, remove the front differential carrier seal assembly (800).
6. Using a brass drift and hammer, drive out the front differential bearing race (647) and the front differential carrier bearing shim-selective.
7. Remove the 1 front differential transfer drive gear assembly bearing retainer bolt (807) and the front differential transfer drive gear assembly bearing retainer (806).
8. Using SA9133T (1) SA9133T-1 (2) and J 26941 (3), remove the front differential transfer drive gear assembly bearing (808).
9. Remove the front differential transfer drive gear front thrust bearing assembly (262).