For 1990-2009 cars

### Removal Procedure

1. Remove the muffler with tailpipe. Refer to Muffler Replacement .
2. Remove the rear exhaust heat shield.
3. Loosen the 3 nuts (arrows).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear exhaust heat shield.

Tighten
Tighten the 3 nuts to 6 N·m (53 lb in).

2. Install the muffler with tailpipe. Refer to Muffler Replacement .