For 1990-2009 cars

## Front Door Inside Handle Rod Replacement Sedan

### Removal Procedure

1. Remove the front side door trim paneling. Refer to Front Side Door Trim Panel Replacement .
2. Partly loosen the water vapor barrier.

• | Remove the 2 front door retainer base inner paneling.

• | Loosen the water vapor barrier in the area of the hatching.

3. Remove the cable from front door inner door actuation.

Remove the cable from bracket.

### Installation Procedure

1. Refit the cable to inner door actuation.

Insert the cable into bracket.

2. Install the water vapor barrier.

Install the 2 front door retainer base inner paneling.

3. Install the front side door trim panel. Refer to Front Side Door Trim Panel Replacement .

## Front Door Inside Handle Rod Replacement Coupe

### Removal Procedure

1. Remove the front side door trim panel. Refer to Front Side Door Trim Panel Replacement.
2. Partly loosen the water vapor barrier.

• | Remove the 2 holding angles.

• | Remove the 2 pins.

3. Remove the front door lock - left side.

• | Remove the 3 bolts.

• | Disconnect the wiring harness plug.

• | Disconnect the 2 connector linkages.

• | Remove the retainer clip.

4. Remove the front door cable inner door actuator.

Remove the cable from bracket.

### Installation Procedure

1. Install the inner front door cable actuator.

Insert the cable into bracket.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the front door lock - left side.

• | Install the 2 connector linkages.

• | Install the retainer clip.

Tighten
Tighten the 3 bolts to 8 N·m (70 lb in).

• | Connect the wiring harness plug.

3. Fasten the water vapor barrier.

• | Install the 2 holding angles.

• | Install the 2 pins.

4. Install the front side door trim panel. Refer to Front Side Door Trim Panel Replacement.