For 1990-2009 cars

### Removal Procedure

1. Remove the bench seat.

• | Unlock the 2 brackets (1) front.

• | Support the 2 bench seats from the rear bracket.

• | Push the seat simultaneously backwards and upward.

2. Remove the upholstery clamp.

Remove the 48 clamps.

3. Loosen the surrounding upholstery.
4. Remove the upholstery clamps from the seat area.

• | Remove the 21 clamps.

• | Remove the upholstery covering.

5. Remove the upholstery padding.

### Installation Procedure

1. Insert the pad.
2. Fasten the upholstery covering on the seat area.

• | Position the upholstery covering.

• | Install the 21 clamps.

3. Place the upholstery covering all the way around.
4. Install the upholstery clamps.

Install the 48 clamps.

5. Install the rear seat.

Insert the rear seat cushion and position.