For 1990-2009 cars

### Removal Procedure

1. Remove the front wheel.
2. Remove the stabilizer shaft links.

• | Remove the stabilizer shaft link (1) from spring strut support tube.

• | Counterhold at the two flattened areas of the knuckle bolt with open-ended wrench.

• | Remove the stabilizer shaft link from stabilizer (2).

• | Counterhold at the two flattened areas of the knuckle bolt with open-ended wrench.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the stabilizer shaft links to the stabilizer.

Tighten
Tighten the nuts to 55 N·m (40 lb ft).

• | Use the 2 new nuts.

• | Counterhold at the two flattened areas of the knuckle bolt with open-ended wrench.

2. Install the stabilizer shaft links to spring strut support tube.

Counterhold at the two flattened areas of the knuckle bolt with open-ended wrench.

Tighten
Tighten the bolt to 55 N·m (40 lb ft).

3. Install the front wheel.

Tighten
Tighten the bolt to 110 N·m (81 lb ft).