For 1990-2009 cars

### Removal Procedure

Note: The selector lever on the transmission must engage in each case: P (most forward position) (2), R, N (1), D, 3, 2, 1.

1. Move the selector lever through all the positions and back again.

• | Change the gear from P to 1.

• | Change the gear from 1 to P.

Warning: Refer to Battery Disconnect Warning in the Preface section.

2. Remove the battery.

• | Disconnect the negative cable (2) from the battery.

| Remove the nut.

• | Disconnect the positive cable (3) from the battery.

| Remove the nut.

• | Remove the bracket (1).

| Remove the bolt (4).

• | Remove the battery.

3. Remove the battery tray.

• | Release the cable tie.

• | Remove the 3 bolts (1).

4. Open the locking clamp (1) on the selector cable.

Open upward with a small screwdriver.

### Installation Procedure

Note: Ensure that the selector lever engages correctly in the P position by moving the selector lever forwards and backwards without pressing the locking button.

1. Adjust the selector cable.

• | Move the selector lever to the P position.

• | Turn the selector lever (1) on the transmission as far as the stop (position P) (2).

• | Engage the pawl in parking lock wheel.

• | Turn the front wheels.

2. Tighten the locking clamp (1) on the selector cable.

Press downwards.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the battery tray.

Fasten the cable tie.

Tighten
Tighten the 3 bolts to 10 N·m (89 lb in).

4. Install the battery.

• | Install the bracket (1).

Tighten
Tighten the bolt (4) to 15 N·m (11 lb ft).

• | Connect the positive cable (3) to the battery.

• | Connect the negative cable (2) to the battery.

5. For programming procedures, refer to Control Module References.