For 1990-2009 cars

### Removal Procedure

1. Remove the outer rear quarter panel molding.

Carefully pry off the molding with a plastic wedge (1).

Important: Ensure that the paint is not damaged.

2. Remove the remaining adhesive.

Remove the remaining adhesive from the molding and the outer rear quarter panel with a molding adhesive remover disk (2).

### Installation Procedure

1. Dimensions 3 door.

| Important: The dimensions II and III are measured starting from the bead in the side sillboard.

• | Front Clearance--Horizontal (I) 3 mm (0.12 in).

• | Rear Clearance--Vertical (II) 213 mm (8.39 in).

• | Front Clearance--Vertical (III) 202 mm (7.95 in).

Important: The adhesive surface must be grease and dust free.

2. Apply the adhesive strips on the molding.
3. Install the outer rear quarter panel molding.