For 1990-2009 cars

### Removal Procedure

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement .
2. Remove the front fascia center support.

Release the 2 (1).

3. Remove the front fascia front guide rail.

Drill out the 3 blind rivets (arrows).

### Installation Procedure

1. Prepare the front fascia front guide rail.
2. Install the front fascia front guide rail.

• | Align the front fascia front guide rails with the center fastening hole.

• | Install the 3 blind rivets.

3. Install the front fascia center support.
4. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement .