For 1990-2009 cars

### Removal Procedure

1. Remove the rear compartment carpet (1).
2. Remove the trailer hitch ball head.

• | Loosen the fastening belt (1).

• | Remove the ball head (2).

3. Remove the rear compartment storage tray--left side.

• | Lift the right storage tray (2).

• | Remove the left storage tray (1).

### Installation Procedure

1. Install the rear compartment storage tray--left side.

Insert the storage tray.

2. Install the trailer hitch ball head.

• | Thread the belt through eye.

• | Insert the ball.

• | Tighten the belt.

3. Install the rear compartment carpet.