For 1990-2009 cars

### Removal Procedure

1. Remove the front floor console. Refer to Front Floor Console Replacement .
2. Remove the selector actuator cable (2) from the selector lever.

• | Remove the retaining clamp (1).

• | Disconnect the selector lever from the bracket.

3. Remove the selector lever assembly.

• | Disconnect the wiring harness plug (1).

• | Remove the 4 bolts (2).

• | Remove the selector lever assembly.

4. Remove the 2 shift lock actuator from the selector lever assembly.

• | Remove the bolt (1).

| Important: Note the configuration of cables.

• | Disconnect the 4 wiring plugs from the shift lock actuator.

5. Remove the 2 shift lock actuator (1) from the bracket (2).

• | Carefully bend the 2 lock outward.

• | Remove the 2 shift lock actuator with the spacer plate (3).

### Installation Procedure

1. Install the 2 shift lock actuator (1) to the bracket (2).

• | Insert the 2 shift lock actuator with the spacer plate (3).

• | The 2 locks must engage.

Notice: Refer to Fastener Notice in the Preface section.

Important: Note configuration of cables.

2. Install the 2 shift lock actuator to the selector lever assembly.

Connect the 4 wiring plugs to the shift lock actuator.

Tighten
Tighten the bolt (1).

3. Install the selector lever assembly.

• | Insert the selector lever assembly.

Tighten
Tighten the 4 bolts (2) to 5 N·m (44 lb in).

• | Connect the wiring harness plug (1).

4. Install the selector actuator cable (2) to the selector lever.

• | Install the selector lever to the bracket.

• | Install the retaining clamp (1).

5. Install the front floor console. Refer to Front Floor Console Replacement .
6. Check the selector lever safety functions.
7. For reprogramming procedures, refer to Control Module References .