For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accelerator Pedal Position Sensor Nuts | 12 N·m | 106 lb in
Air Cleaner Assembly Bolt | 5 N·m | 44 lb in
Air Intake Pipe to Air Mass Flow Meter | 3.5 N·m | 31 lb in
Barometric Pressure Sensor Bolts | 5 N·m | 44 lb in
Battery Ground Connection Nut | 5 N·m | 44 lb in
Battery Nut | 5 N·m | 44 lb in
Camshaft Position Actuator Solenoid Bolts | 6 N·m | 53 lb in
Camshaft Position Sensor of the Exhaust Camshaft | 6 N·m | 53 lb in
Camshaft Position Sensor of the Intake Camshaft | 6 N·m | 53 lb in
Crankshaft Position Sensor Bolt | 4.5 N·m | 40 lb in
Engine Control Module Bolts | 8 N·m | 71 lb in
Engine Control Module Ground Cable Bolt | 8 N·m | 71 lb in
Fuel Filler Tube Clamp | 3.5 N·m | 31 lb in
Fuel Line Bracket Bolts | 5 N·m | 44 lb in
Fuel Rail Bolts | 8 N·m | 71 lb in
Fuel Tank Holding Strap Bolts | 23 N·m | 17 lb ft
Ground Clamp Nut | 5 N·m | 44 lb in
Ground Clamp to Ground Terminal Nut | 5 N·m | 44 lb in
Ground Clamp to Negative Terminal Nut | 5 N·m | 44 lb in
Ground Connection Nut | 5 N·m | 44 lb in
Heat Shield Nuts | 8 N·m | 71 lb in
Intake Manifold Support Bolts | 8 N·m | 71 lb in
Intermediate Fuel Pipe Bracket Bolts | 2.5 N·m | 22 lb in
Knock Sensor Bolt | 20 N·m | 15 lb ft
Manifold Absolute Pressure Sensor Bolt | 8 N·m | 71 lb in
Mass Airflow Sensor Clamps | 3.5 N·m | 31 lb in
Oxygen Sensor | 40 N·m | 30 lb ft
Pressure Sensor Bolt | 2.5 N·m | 22 lb in
Spark Plugs | 25 N·m | 18 lb ft
Throttle Valve Assembly Bolts | 8 N·m | 71 lb in
Wheel Bolts - Rear | 110 N·m | 81 lb ft
Wheel Housing Inner Paneling Bolts/Nuts - Right Rear | 2.5 N·m | 22 lb in