For 1990-2009 cars

### Removal Procedure

1. Lower the molded headlining. Refer to Headlining Trim Panel Replacement .
2. Remove the sunroof module assembly. Refer to Sunroof Module Assembly Replacement .
3. Remove the window outer seal.

Remove the window outer seal from the guide.

### Installation Procedure

Important:

• | Position the window outer seal with the sunroof in the front area on markings (2).

• | Cut off the window seal at the lower area of the opening of the sunroof (3).

1. Install the window outer seal (1).

1.1. | Insert the window outer seal into the guide.

1.2. | Cut off the extra window seal and glue the end to the abutting seal (4) (super glue).

2. Install the sunroof module assembly. Refer to Sunroof Module Assembly Replacement .
3. Install the molded headlining. Refer to Headlining Trim Panel Replacement .