For 1990-2009 cars

### Removal Procedure

1. Remove the upper extension trim panel (1).

• | Release the 3 clips.

• | Remove the foam.

• | Disconnect the wiring harness plug (3).

2. Release the front door upper speaker (2).

### Installation Procedure

1. Install the front door upper speaker.
2. Install the upper extension trim panel.

• | Connect the wiring harness plug.

• | Replace the foam.