For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Remove the air cleaner assembly (1).

2.1. | Disconnect the mass air flow sensor wiring harness plug (4).

2.2. | Remove the bolt (2).

2.3. | Remove the air intake pipe (3) from the throttle valve module.

2.4. | Release the clamp.

2.5. | Remove the air intake pipe (5).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the air cleaner assembly.

Tighten
Tighten the bolt to 5 N·m (44 lb in).

1.1. | Install the air intake pipe to the air mass flow meter.

Tighten
Tighten the clamp to 3.5 N·m (31 lb in).

1.2. | Install the air intake pipe.

1.3. | Connect the mass air flow meter wiring harness plug.

2. Close the hood.