For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Remove the positive crankcase ventilation pipe (1).

• | Disconnect the wiring trough (2) from the cylinder head cover.

• | Disconnect the 2 quick-release fittings.

### Installation Procedure

1. Install the positive crankcase ventilation pipe.

• | Connect the 2 quick-release fittings.

• | Connect the wiring harness to the cylinder head cover.

2. Close the hood.