For 1990-2009 cars

### Removal Procedure

1. Position the transmission control lever into 4th gear.
2. Release the bolt (1) for the relay point clamp.

Disconnect the relay point from the selector lever lever.

3. Disconnect the selector lever boot (2) from the bulkhead.

### Installation Procedure

Important: Push the lever boot onto the gearshift rod without twisting it.

1. Attach the selector lever boot (2) to the bulkhead.

Important: Do not tighten the clamping screw (1).

2. Attach the transmission relay point to the selector lever.
3. Adjust the transmission selector lever link. Refer to Selector Lever Link Adjustment .