For 1990-2009 cars

### Removal Procedure

1. Remove the hood. Refer to Hood Replacement.
2. Remove the air inlet screen. Refer to Air Inlet Screen Replacement.
3. Remove the right (I) and left (II) hood hinges.

• | Remove the 3 bolts (1).

• | Remove the 3 bolts (2).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the hood hinge.

Tighten
Tighten the 6 bolts to 20 N·m (15 lb ft).

2. Install the air inlet screen. Refer to Air Inlet Screen Replacement.
3. Install the hood. Refer to Hood Replacement.